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Viscous oil inflow control device for equalizing screen flow
www.google.com.co/patents/US7578343
Grant - Filed 23 Aug 2007 - Issued 25 Aug 2009 - Jody R. Augustine -
== aer Hughes Incorporated
at least one flow control device in at least one of said sections in flow
said passage is unobstructed along its length. ... for a specific job and
then quickly welded to the base pipe 10 afier the openings 12 are properly
located. .. The use of an annular flow path also reduces risk of clogging
from solids that
Overview - Related - Discuss

Sand control screen assembly having integral connector ...

www.google.com.co/patents/US8430158
Grant - Filed 30 Aug 2010 - Issued 30 Apr 2013 - Luke Wiliam Holderman
- Halliburton Energy Services, Inc.

@)~ VVtout imiing the scope of the present nvention, its background wil
be .. For example, the material used for the base pipe may be 13 chrome
while the ... Due to the dificulty of the welding process and the post-weld
heat ... Together, the housing sections create a generally annular fluid
flow path between
Overview - Related - Discuss

Sand control screen assembly having remotely disabled ...
www.google.com.co/patents/US8256522

Grant - Filed 15 Apr 2010 - Issued 4 Sep 2012 - Jan Veit - Halliburton
Energy Services, Inc.

Aflow control screen having a fluid flow path between a perforated
section o ... Original Assignee, Halliburton ... 3A-3C are cross sectional
Views of a valve assembly in its various operating configurations that is
operable for use in a flow ... which is preferably welded to base pipe 102





