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Google Patents Q
SEARCH TERMS About 5,505 results ordered by relevance, grouped by classification (view ungrouped)
aldehyde x
co9D1?
scavenger X Coating compositions, e.g. paints, varnishes or lacquers, based on

inorganic substances

Use of aldehyde scavengers in interior building products
‘Application CA2841821A1 - Runhai Lu - Usg Interiors, Lic:
- Priority 2011-07-21 - Fled 2012:07-17 + Published 2013.01-24
A coating for application to the surface of an interior building product comprises: a resin formulation such as a
melamine formaldehyde resin characterized by ts ability to strengthen the interior building product when applied
SEARCH FIELDS 5 3 coating to the building product; and an aldehyde scavenger selected from

building product X

Functional construction board

Grant CN100575066C - % # i1k - RE&HASH

Priority 2007-02-02 - Fled 2007-11-16 Granted 20091230

Building plate according to claim 2, characterized in that the aldehyde scavenger to capture formaldehyde and

acetaldehyde. 4.... Also, typically, several layers of the building panel is coated process and as product design, but
MORE v still exist because the final step to the top of this painting has been caused by

> search within classification C09D1 (1,101 results)

Method for producing a wood based product

‘Application WO2006033613A1 + Tomas Erik Peter Svanholm + Akzo Nobel Coatings Int By

Priority 2004-09-20 - Fled 2005-09-15 - Published 2006-03-30

Emission of aldehydes, especially formaldehyde, from products such as flooring materials, furniture materials and

Bl W02013012828.pdf ¥ Mostrar todas las descargas.. X
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Inorganic fiber mat and method for production thereof

‘Application US20040028576A1 + Yoshifumi Mizuno - Yoshifumi Mizuno

Priority 2001-08-20 - Fled 2002-08-16 + Published 2004-02.12

The aldehyde scavenger is applied between the application of the binder and the curing by polymerization.
[0004] Aldehyde emissions after completion of building constructions are low enough to do no harm to human
bodies. ... [0043] The aldehyde scavenger in the present invention is added so that the pickup of the aldehyde
[ ‘scavenger and its reaction product is from 3 to 15 parts by mass in relation

building product X

() Before priority date 2011-07-21 x By-product absorbers for oxygen scavenging systems

Grant US5942297A - Drew Ve Speer » Cryovac, Inc.
Priority 1996-03-07  Filed 1996-03-07 Granted 1999-08-24
The article of claim 1 wherein the third layer comprising the by-product absorber is between the second layer
‘comprising an oxygen scavenger and an oxygen sensitive product. 3. An article for packaging an oxygen sensitive

MORE product ... Aldehyde-absorbing layers made of polyalkylene imines are known for incorporation into polyethylene
and polypropylene films as a method of reducing the build-up of oildegradation by-products from snack foods,
see US. Pat. No. 5,284,892 issued to Brodie et al., Feb.

Functional construction board

Grant CN100575066C - % # i1k - RE&HASH

Priority 2007-02-02 - Fled 2007-11-16 Granted 20091230
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Inorganic fiber mat and method for production thereof

Abstract

‘The present invention provides an inorganic fiber mat with  low aldehyde emission without
detriment to various physical properties of inorganic fiber mats and a process for its production.
An inorganic fiber mat formed by bonding inorganic fibers together with a binder comprising a
phenol resin as a main component, wherein the inorganic fiber mat comprises an aldehyde
‘scavenger and its reaction product in an amount of from 3 to 15 parts by mass in relation to 100
parts by mass of the binder pickup, and the aldehyde scavenger is at least one member selected
from the group consisting of the sodium salts, potassium salts and calcium satts of sulfurous acid,
acidic sulfurous acid, ithionous acid and disulfurous acid. The aldehyde scavenger is applied
between the application of the binder and the curing by polymerization
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Original document Claims of EP1291389 (A2)
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INPADOC legal status members:
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“patent iransiate” button?
-+ How can | view the claim

structure? 1. Alow formaldehyde emission coating composition comprising:
-+ Why are the claims sometimes in
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-+ How can [ search in the textof

the claims? 2.The coating of claim 1, wherein the polyamide is a synthetic polyamide.
-+ How can | view chemical

Structures in the ful text? 3.The coating of claim 2, wherein the synthetic polyamide is selected from the group consisting essentially of polyacrylamides,
-+ Whatis Global dossier? polymethacrylamides, polyamide telomers, N-substituted polyamides and combinations thereof.

4.The coating of claim 1, wherein the polyamide is a protein
5. The coating of claim 4, wherein the protein is selected from the group consisting of casein, soy protein and combinations thereof.

6.The coating of claim 1, wherein the formaldehyde resin is selected fom the group consisting of melamine formaldehyde, urea
formaldehyde, phenol formaldehyde and combinations thereof.

7.The coating of claim 1, further including at least one of the components selected from the group consisting of catalysts, filers, surfactants, -

&) 13247107--00000000..TF |~ ¥ Mostrar todas las descargas.. X





 [image: image5.png]B0 About thisfile - European X ) |E! Espacenet - Bibliographic x \ [ traslate - Buscar con Gooc x { [ aldehyde, reduction, resi x \\ |\ W R R ) e

€ | [3 worldwide.espacenet.com/publicationDetails/biblio?CC=US&NR=2010037399&KC=8&locale=en_EP&FT: | =
Europisches -
Deutscn Engish  Frangais
Espacenet
P Contact
il
Office européen ‘Change country
e
£P0 oni
e 1] e ey e | |
Bibliographic data: US2010037399 (A1) — 2010-02-18
Bbograri: duta! Y inmypatents list @ Global Dossier I Reportdata eror & Print
Descripton
Glams
Aldehyde reduction in aqueous coating and leather finishing compositions
gl document
Page bookmark _ US201003736 (A1) - Aldehyce eguction I aqueous coaling and leaher inishing comgosiions
Citing documents Inventor(s): HOEFLER JOSEPH M [US]; KLEIN KELLEY L [US], OTTINGER JILL A [US] +
INPADOC legal status Applicant(s): HOEFLER JOSEPH M, ; KLEIN KELLEY L, ; OTTINGER JILL A, ; ROHM AND HAAS COMPANY
(R Gl L Classification: -international: B05D3/02; C14C11/00
“cooperative: BOSDIIZ; C14C11003; BOSDIAQT
Guick heip -
‘Applcation number: US20060228345 20080812
> et et oy o aualy
{extas facsimile? Priority number(s): US20080228348 20080812
+ i does At 20 A ana
Stand for afera European Aiso published as: [ USa234021 (B2
Sublcaion unber:
-+ Wnatnappens rlclck on g
Latenis st
»Wniihampers sicikontie Abstract of US2010037398 (A1)
Reqsier buton?
*:V" ‘afe‘sﬂéﬂ;: S‘ﬂs:afﬂ tions Translate this textinto [1]
documenis? [EETAJ - 2 or1r2nslato [ESEIE
-» Howcan | oomar s pace
iy does s stofcocuments  Tne presentinvention rovides methodsfrreducing he leve ffee aicehydes n coaings forfexile substrates, such as tanned latner,
i i nading Also pUlsned  and Subsaialy S0Sh)oS Toe SubSTateS The methods Comp1Se apBNG & 1 SUbSUAe & composiion of one o more aqusos smgion
25~ somelimes appear and whal of suspandion composiian o an aGrlc poymerorSicon contaNNG paymer hat s made flom.of conains e of mors ower aky lconal
S tese documents? or degraces on slorage o It uss o ot uch an lcahol, And One o More walr-nsaluble o Sighty wate solupla ldenyce scavenger
-+ dosomeimes ind e compouna.allowed by 4G or cUrin e applied compostion o o acoatna In addfon he methods povide ennanced aden)ce
‘absiactofa corespondin SErubbing,sspecially for acetaldenycs, oy apaing 1o 3 subsrate an aqusaus aerylc poymer o iican contaning poymer smulsion or
document? suspension comorising a aldehvde scavenaer comoound that is substantiallv deorotonated. i.. by raisina the oH comoosition to 5.5 or M

(& 13247107--00000000...TIF

¥ Mostrar todas las descargas.. X





[image: image6.png]polivin, x Y US200¢

/B About x VE Espace: x V020100 x Y E Espace x V[E20100: x V [E Espace x Y [T 201002 x \ & Alcoho x ¥ P Alcohc x V[ Pintura x \ [ wwwse x V[ Manue x \ [ Pinturz x|
€ - C | @ https//patents.google.com/?q=polivinyl+alcohol&:q=formaldehyde-based + resins&before=20110721 R =

GOOgle Patents Q [+} s

‘SEARCH TERMS ‘About 29,060 results ordered by relevance, grouped by classification (view ungrouped)

polivinyl alcohol X

formaldehyde-based resins X Pulp or paper, comprising cellulose or lignocellulose fibres of
natural origin only

Poly (vinyl alcohol) - based formaldehyde-free curable aqueous composition
— Application US20060252855A1 - Elena Pisanova - Dynea Austria Gmbh
= Priority 2005-05-06 - Filed 2006-05-05 - Published 2006-11-09
A formaldehyde-free curable aqueous composition containing polyvinyl alcohol, a mult-functional
crosslinking agent, and, optionally, a catalyst. .. These formaldehyde based resins are inexpensive,
() seforeprioity date 20110721 x ‘have low viscosity, and are able to cure to form a rigid polymer, thereby providing the finished
product

‘SEARCH FIELDS

Inorganic fillers modified with vinyl alcohol polymer and cationic melamine ...
Grant US4495245A - David W. Zunker « E. 1. Du Pont De Nemours And Company

Priority 1983.07-14 « Fled 1983.07-14 Granted 19850122

“This invention relates to filers and more specifically it relates to fillers modified with polyvinyl
alcohol and cationic melamine-formaldehyde resin. 2..... Cationic melamine-formaldehyde resin
‘adsorbed onto the filer can range from about 0.01% to about 3.0%, based on dy filler weight, with
from about

MORE v

Process of preparing corrugated paper board with a particular polyvinyl .

Grant US4094718A - Edward Peter Czerwin - E. . Du Pont De Nemours And Company

Priority 19751117 « Fled 19751117 Granted 19780613

Improved polyvinyl alcohol modified starch-based corrugating adhesive is provided by employing a
fine particle size, low cold water solubles .. from the group consisting of urea/formaldehyde resins,
ketone/formaldehyde resins, melamine/formaldehyde resins and resorcinol formaldehyde resi
6

Cationic polyvinyl alcohol binder additive

Grant US5147908A - Wiliam C. Floyd - Sequa Chemicals Inc

Priority 1990-09-24 - Filed 1990-09-24 Granted 1992-09-15

reaction product of an aqueous solution of a blocked glyoxal resin, a cationic water-soluble aldehyde -
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